# ESRI C++ code assignment

## Requirements

The requirements specification is provided in `assignment.pdf`.


## Design remarks

For sake of simplicity most of validation and error handling is performed during
loading the input files.


## Setup

Execute the bash script `install_deps.sh` on a Debian GNU/Linux system to install
the required dependencies.

The protobuf dependencies are installed as Debian packages. All other dependencies
are installed using the CMake FetchContent feature.

## Build

Execute the bash script `build.sh` to perform both build and testing steps.

The overall process is implemented using CMake. The application artifact is located
at `build/src/main`.


## Usage

The command-line parameters can be passed as follows:
```
main <input-file[s]> <json-ouput-file>
```

* At least one *input-file* and *json-ouptut-file* must be provided.
* Multiple *input-files* are supported.


## Links
* Protobuf
  * https://developers.google.com/protocol-buffers/docs/cpptutorial
  * https://github.com/protocolbuffers/protobuf/tree/master/examples
  * https://cmake.org/cmake/help/latest/module/FindProtobuf.html
* Json C++ library
  * https://github.com/nlohmann/json
* Catch2 unit testing framework
  * https://github.com/catchorg/Catch2
